IDA SDK

- Main Page
- Header Files
- Classes
- Modules

Macros
Internal breakpoint properties

## Detailed Description

Used by bpt_t::props.

## Macros
#define | BKPT_BADBPT 0x01
| failed to write the bpt to the process memory (at least one location)
#define | BKPT_LISTBPT 0x02
| include in bpt list (user-defined bpt)
#define | BKPT_TRACE 0x04
| trace bpt; should not be deleted when the process gets suspended
#define | BKPT_ACTIVE 0x08
| active?
#define | BKPT_PARTIAL 0x10
| partially active? (some locations were not written yet)
#define | BKPT_CNDREADY 0x20
| condition has been compiled
#define | BKPT_FAKEPEND 0x40
| fake pending bpt: it is inactive but another More...
#define | BKPT_PAGE 0x80
| written to the process as a page bpt. More...

## Macro Definition Documentation

#define BKPT_FAKEPEND 0x40

fake pending bpt: it is inactive but another

bpt of the same type is active at the same address(es)

#define BKPT_PAGE 0x80

written to the process as a page bpt.

is available only after writing the bpt to the process.