IDA SDK

- Main Page
- Header Files
- Classes
- Modules

Macros
Assembler feature bits

## Detailed Description

Used by asm_t::flag.

## Macros
#define | AS_OFFST 0x00000001L
| offsets are 'offset xxx' ?
#define | AS_COLON 0x00000002L
| create colons after data names ?
#define | AS_UDATA 0x00000004L
| can use '?' in data directives
#define | AS_2CHRE 0x00000008L
| double char constants are: "xy
#define | AS_NCHRE 0x00000010L
| char constants are: 'x
#define | AS_N2CHR 0x00000020L
| can't have 2 byte char consts
#define | AS_1TEXT 0x00000040L
| 1 text per line, no bytes
#define | AS_NHIAS 0x00000080L
| no characters with high bit
#define | AS_NCMAS 0x00000100L
| no commas in ascii directives
#define | AS_HEXFM 0x00000E00L
| mask - hex number format
#define | ASH_HEXF0 0x00000000L
| 34h
#define | ASH_HEXF1 0x00000200L
| h'34
#define | ASH_HEXF2 0x00000400L
| 34
#define | ASH_HEXF3 0x00000600L
| 0x34
#define | ASH_HEXF4 0x00000800L
| $34
#define | ASH_HEXF5 0x00000A00L
| <^R > (radix)
#define | AS_DECFM 0x00003000L
| mask - decimal number format
#define | ASD_DECF0 0x00000000L
| 34
#define | ASD_DECF1 0x00001000L
| #34
#define | ASD_DECF2 0x00002000L
| 34.
#define | ASD_DECF3 0x00003000L
| .34
#define | AS_OCTFM 0x0001C000L
| mask - octal number format
#define | ASO_OCTF0 0x00000000L
| 123o
#define | ASO_OCTF1 0x00004000L
| 0123
#define | ASO_OCTF2 0x00008000L
| 123
#define | ASO_OCTF3 0x0000C000L
| @123
#define | ASO_OCTF4 0x00010000L
| o'123
#define | ASO_OCTF5 0x00014000L
| 123q
#define | ASO_OCTF6 0x00018000L
| ~123
#define | ASO_OCTF7 0x0001C000L
| q'123
#define | AS_BINFM 0x000E0000L
| mask - binary number format
#define | ASB_BINF0 0x00000000L
| 010101b
#define | ASB_BINF1 0x00020000L
| ^B010101
#define | ASB_BINF2 0x00040000L
| %010101
#define | ASB_BINF3 0x00060000L
| 0b1010101
#define | ASB_BINF4 0x00080000L
| b'1010101
#define | ASB_BINF5 0x000A0000L
| b'1010101'
#define | AS_UNEQU 0x00100000L
| replace undefined data items with EQU (for ANTA's A80)
#define | AS_ONEDUP 0x00200000L
| One array definition per line.
#define | AS_NOXRF 0x00400000L
| Disable xrefs during the output file generation.
#define | AS_XTRNTYPE 0x00800000L
| Assembler understands type of extern symbols as ":type" suffix.
#define | AS_RELSUP 0x01000000L
| Checkarg: 'and','or','xor' operations with addresses are possible.
#define | AS_LALIGN 0x02000000L
| Labels at "align" keyword are supported.
#define | AS_NOCODECLN 0x04000000L
| don't create colons after code names
#define | AS_NOTAB 0x08000000L
| Disable tabulation symbols during the output file generation.
#define | AS_NOSPACE 0x10000000L
| No spaces in expressions.
#define | AS_ALIGN2 0x20000000L
| .align directive expects an exponent rather than a power of 2 More...
#define | AS_ASCIIC 0x40000000L
| ascii directive accepts C-like escape sequences More...
#define | AS_ASCIIZ 0x80000000L
| ascii directive inserts implicit zero byte at the end

## Macro Definition Documentation

#define AS_ALIGN2 0x20000000L

.align directive expects an exponent rather than a power of 2

(.align 5 means to align at 32byte boundary)

#define AS_ASCIIC 0x40000000L

ascii directive accepts C-like escape sequences

(\n,\x01 and similar)